Safety Come First - Comply or Die

We are extremely focused on all risk aspects! We managed successfully to conduct the race in 2021 without any risk for the spectators and the riders/drivers. Our intention is to build on this track record going forward.

***NEW REQUIREMENTS FOR 2022 !!!***

We have defined a few MANDATORY requirements that all vehicles and drivers MUST comply with to race.

**The vehicles**

* Pre-war cars, coupe, roadsters and specials.
* Pre-war bikes, US or European.
* Appearance, main parts and performance parts must not be newer than year 1947.

**The Motorcycle Riders**

* Modern pilot helmet (make it look old, is ok) – NEW to 2022
* All riders must be wearing a back shield – NEW for 2022
* All riders must be wearing gloves when racing – NEW for 2022
* Googles, Glasses or Face shield. \*
* Shoes or boots with firm sole. \*
* Long pants or jeans. \*
* Jacket or jersey. \*
* Not affected by alcohol, drugs or medicine.
* *\* Clothing needs to be period correct.*

**The driver**

* Helmet
* Googles, Glasses or Face shield. \*
* Shoes or boots with firm sole. \*
* Long pants or jeans. \*
* Jacket or jersey. \*
* Not affected by alcohol, drugs or medicine.
* *\* Clothing needs to be period correct.*

**Disqualification will occur if:**

* Drivers, mechanics or helpers are under influence of alcohol or drugs.
* Failing to follow the guidelines and directions from the official RMF team.
* Reckless or irresponsible driving at all times. (Rømø beach is considered a public road)

Safety and technical requirements

**Engine compartment:**

* Engine needs to be clean.
* Gasoline / Petrol lines and/or hoses need to be fastened.
* The gasoline / petrol lines or system must not leak.
* Oil must not leak out - sweating is allowed.
* No loose components.
* No loose items.
* Seats need to be fastened.
* Fire extinguisher within reach.

**Vehicle exterior:**

* Racing number must be visible.
* All body panels, hood, trunk etc. needs to be secured.
* Headlights needs to be removed or the glass secured.
* Petrol / gas tank needs to be secured.
* Gas cap in place and secured.
* Hub caps either off or secured.
* Steering linkage needs to be secured.
* Wheels checked and secured.
* Tire (street or racing) must be intact. No paddle and/or tractor styled tires.
* No cracks in the frame.

These requirements can also be downloaded as a word file here: [Download](https://www.romomotorfestival.com/misc/Safety-and-Technical-requirements-2018-ver-1.0.doc)  
  
Thank you!  
FIA/DMU/AMK/DASU/MSS & Rømø Motor Festival